/****************************************************************************
**
** Copyright (C) 2018 Blackberry
** Contact: Blackberry (qt@blackberry.com)
** Contact: KDAB (info@kdab.com)
**
** Copyright (C) 2021 The Qt Company Ltd.
** Contact: https://www.qt.io/licensing/
**
** This file is part of the Qt Creator documentation.
**
** Commercial License Usage
** Licensees holding valid commercial Qt licenses may use this file in
** accordance with the commercial license agreement provided with the
** Software or, alternatively, in accordance with the terms contained in
** a written agreement between you and The Qt Company. For licensing terms
** and conditions see https://www.qt.io/terms-conditions. For further
** information use the contact form at https://www.qt.io/contact-us.
**
** GNU Free Documentation License Usage
** Alternatively, this file may be used under the terms of the GNU Free
** Documentation License version 1.3 as published by the Free Software
** Foundation and appearing in the file included in the packaging of
** this file. Please review the following information to ensure
** the GNU Free Documentation License version 1.3 requirements
** will be met: https://www.gnu.org/licenses/fdl-1.3.html.
** $QT_END_LICENSE$
**
****************************************************************************/

/*!
    \previouspage creator-developing-mcu.html
    \page creator-developing-qnx.html
    \nextpage creator-setup-webassembly.html

    \title Connecting QNX Devices

    You can connect QNX devices to the development PC to deploy, run and debug
    applications on them from within \QC. The QNX Neutrino RTOS should provide
    a few additional command line tools and services, as described in
    \l {Qt Creator Target Requirements}.

    \note In Qt 6, Qt for QNX is a part of
    \l{https://doc.qt.io/QtForDeviceCreation/index.html}{Qt for Device Creation},
    and the \QC support is considered experimental.

    \section1 Adding a QNX Neutrino Device in \QC

    Adding a QNX Neutrino device is very similar to
    \l{Connecting Generic Remote Linux Devices}, except that
    you need to select \uicontrol {QNX Device} in the
    \uicontrol {Device Configuration} wizard.

    \section1 Adding Kits for QNX Devices

    To view QNX device settings, select \uicontrol Tools > \uicontrol Options >
    \uicontrol Devices > \uicontrol QNX. Select the \uicontrol {Generate kits}
    check box to allow \QC to generate kits for QNX development. For more
    information about how to create the kits manually, see \l {Adding Kits}.
*/
